
Important Notice

* The Safe is **NOT** supplied with an over-ride key
* It is therefore important to insert the batteries and set the user code user the instructions supplied, **before closing the door**
* If the door is accidentally closed before inserting the batteries, connect a 9v battery to the battery port. Whilst holding this in place, touch the screen and enter the pre-set factory code 1,2,3,4 and press the key button ()



* Now set the user code, using the instructions in the user manual